TODO list for smartmontools:

$Id: TODO,v 1.47 2004/02/23 20:32:12 ballen4705 Exp $

SATA devices
------------
Currently work OK if you use the standard IDE drivers in
drivers/ide. If you use the new libata drivers, it won't work
correctly because libata doesn't yet support the needed
ATA-passthrough ioctl() calls. Jeff Garzik, the libata developer, says
that this support will be added in the future. When this happens, add
support to smartmontools for a new SATA/libata device type '-d sata'.

USB devices
-----------
Some USB devices can hang smartctl or smartd.  This is because these
devices fail to comply with SCSI specifications for their packet
command sets.  Work on improving the detection and bail-out procedures
for these flawed devices, so that the user sees an informative error
message and smartd/smartctl don't hang.

ATA-4 (no kidding!)
-------------------
smartctl: add another -t TESTTYPE option to accomodate old-style ATA-4
IBM disks (ATA-4 has no self-test commands). See IBM S25L-2426-02 OEM
HARD DISK DRIVE SPECIFICATIONS for DBCA-203240/204860/206480 2.5-Inch
Hard Disk Drive with ATA Interface Revision (1.0)
http://www.hgst.com/tech/techlib.nsf/techdocs/85256AB8006A31E587256A7D00642A1D/$file/dbca_sp.pdf
section 12.30.1.5 for details.  These disks offer no self-test option,
and the -t offline command only tests a small part of the disk (a
'segment').  We need a -t multioffline that:
 (1) issues auto offline immediate command (tests ONE segment)
 (2) waits until estimated completion time
 (3) tests if off-line data collection status is set to 0x02 (all
     segments completed)
 (4) if not, return to (1)

ATA-6/7
-------
Support selective self-tests (requires an HDIO_DRIVE_TASKFILE ioctl()
interface).

Support extended error logs

Support extended self-test logs

smartctl/smartd
---------------
Add additional -v options (corresponding to comments in
atacmds.c:ataPrintSmartAttribName().

Add interface to Megaraid ATA RAID controllers (Erik)

smartctl: 
---------
Perhaps modify the -q option (quiet mode) so that it only warns of ATA
errors if they have (say) taken place in the last 168 hours (week).

Parse and print additional Attribute flag meanings (IBM ones, eg
performance etc).

smartd:
-------
Perhaps change <nomailer> special argument to -m to have also
<nomailer_fork> which would actually work with -M exec to run the
executable/script in the background rather than in the foreground.
But let's wait for someone to request this. At that point we should
probably use fork/exec rather than system().

Perhaps change smartd to look in /proc/ide and /proc/scsi to see what
exists? If something doesn't exit then don't try to open it?  This
should probably be the default option if there is no configuration
file.

Add ability to monitor "worst" value from attributes (sometimes it
gets larger!) and to monitor the threshold value (sometimes it
changes!).

Add command line option that scans devices then WRITES
/etc/smartd.conf, perhaps as /etc/smartd.conf.output, just for devices
that can be monitored.

FreeBSD
-------
Get interface for 3ware Escalade controllers working (Eduard).
Modify smartctl -h examples

Packaging
---------
Under freebsd and solaris, the following are wrong:
smartd.conf: has linux device paths
smart*.in  : man pages have (mostly) linux device paths
