eCos User Guide
Prev | Appendix A. Target Setup | Next

# TX49 Hardware Setup

The eCos installation CD contains a copy of the eCos GDB stubs in SREC format which must be programmed into the board’s FLASH memory.

## Preparing the GDB stubs

These stub preparation steps are not strictly necessary as the eCos distribution ships with pre-compiled stubs in the directory `loaders/tx49-ref4955` relative to the installation root.

### Building the GDB stub image with the eCos Configuration Tool

1. Start with a new document - selecting the File->New menu item if necessary to do this.

2. Choose the Build->Templates menu item, and then select the TX49 REF4955 hardware.

3. While still displaying the Build->Templates dialog box, select the stubs package template to build a GDB stub. Click OK.

4. Build eCos stubs using Build->Library.

5. When the build completes, the image files can be found in the bin/ subdirectory of the install tree. GDB stub images have the prefix gdb_module.

### Building the GDB stub image with ecosconfig

1. Make an empty directory to contain the build tree, and cd into it.

2. To build a GDB stub ROM image, enter the command:

       $ ecosconfig new ref4955 stubs

3. Enter the commands:

       $ ecosconfig tree
       $ make

4. When the build completes, the image files can be found in the bin/ subdirectory of the install tree. GDB stub images have the prefix gdb_module.

## Installing GDB stubs into FLASH

Boot into the board’s firmware in little-endian mode:

Set the switches like this:

SW1: 10000000 (first lever up, the rest down) SW2: 10000010

Connect serial cable on the lower connector, configure terminal emulator for 38400, 8-N-1.

When booting the board, you should get this prompt:

    HCP5 rev 0.9B .
    HCP5?

Select o (option), a (FLASH) and b (boot write). You should see this:

    Boot ROM Write
    ROM address-ffffffffbd000000, Boot Bus-[32bit]
    ID2 0 4 ffffffffa002ad40
    zzz SS-40000 IV-1 CS-20000 CC-2
    Flash ROM-[28F640J5], [16bit chip] * 2 * 1
    Block size-00040000  count-64
    ROM adr ffffffffbd000000-ffffffffbe000000  mask-00fc0000
    Send Srecord file sa=00000000 size=ffffffffffffffff
    ra=fffffffffe000000

Now send the stub SREC data down to the board using the terminal emulator’s ‘send ASCII’ (or similar) functionality.

Red Hat has experienced some sensitivity to how fast the data is written to the board. Under Windows you should configure Minicom to use a line delay of 100 milliseconds. Under Linux, use the slow_cat.tcl script:

    % cd BASE_DIR/packages/hal/mips/ref4955/<version>/misc
    % slow_cat.tcl < [path]/gdb_module.srec > /dev/ttyS0

Power off the board, and change it to boot the GDB stubs in big-endian mode by setting the switches like this:

SW1: 00000000 (all levers down) SW2: 10001010

The GDB stubs allow communication with GDB using the serial port at connector PJ7A (lower connector). The communication parameters are fixed at 38400 baud, 8 data bits, no parity bit and 1 stop bit (8-N-1). No flow control is employed. Connection to the host computer should be made using a straight through serial cable.

Prev | Home | Next
TX39 Architectural Simulator Setup | Up | VR4300 Hardware Setup