eCos Reference Manual
Prev | Chapter 5. Installation and Testing | Next

# ARM/ARM7+ARM9 ARM Integrator

## Overview

RedBoot supports both serial ports for communication and downloads. The default serial port settings are 38400,8,N,1.

The following RedBoot configurations are supported:

Configuration | Mode | Description | File
--- | --- | --- | ---
ROM | [ROM] | RedBoot running from the board's flash boot sector. | redboot_ROM.ecm
RAM | [RAM] | RedBoot running from RAM with RedBoot in the flash boot sector. | redboot_RAM.ecm
ROMRAM | [ROMRAM] | RedBoot running from RAM, but contained in the board's flash boot sector. | redboot_ROMRAM.ecm

## Initial Installation

RedBoot is installed using the on-board bootPROM environment. See the user manual for full details.

## Quick download instructions

Here are quick start instructions for downloading the prebuilt Redboot image:

- Set DIP switch S1[1] to the ON position and reset or power the board up. You will see the bootPROM startup message on serial port A (J14):

      Initialising...

      ARM bootPROM [Version 1.3] Rebuilt on Jun 26 2001 at 22:04:10
      Running on a Integrator Evaluation Board
      Board Revision V1.0, ARM966E-S Processor
      Memory Size is 16MBytes, Flash Size is 32MBytes
      Copyright (c) ARM Limited 1999 - 2001. All rights reserved.
      Board designed by ARM Limited
      Hardware support provided at http://www.arm.com/
      For help on the available commands type ? or h
      boot Monitor >

- Issue the FLASH ROM load command:

      boot Monitor > L
      Load Motorola S-Records into flash

      Deleting Image 0

      The S-Record loader only accepts input on the serial port.
      Type Ctrl/C to exit loader.

- Either use the ASCII transmit option in the terminal emulator, or on Linux, simply cat the file to the serial port:

      $ cat redboot.srec > /dev/ttyS0

  When complete, type Ctrl-C and you should see something similar to:

      ................................
      ................................
      ....................
      Downloaded 5,394 records in 81 seconds.

      Overwritten block/s
          0

      boot Monitor >

- Set DIP switch S1[1] to the OFF position and reboot the board and you should see the RedBoot banner.

## Special RedBoot Commands

None.

## Memory Maps

RedBoot sets up the following memory map on the Integrator board.

> NOTE: The virtual memory maps in this section use a C and B column to indicate whether or not the region is cached (C) or buffered (B).

    ARM7TDMI
    --------

    Physical Address Range  C B  Description
    ----------------------- - -  -----------
    0x00000000 - 0x0007ffff N N  SSRAM
    0x00080000 - 0x0fffffff N N  SDRAM (depends on part fitted)
    0x10000000 - 0x1fffffff N N  System control and peripheral registers
    0x20000000 - 0x23ffffff N N  Boot ROM (contains boot Monitor)
    0x24000000 - 0x27ffffff N N  FLASH ROM (contains RedBoot)
    0x28000000 - 0x2bffffff N N  SSRAM echo area
    0x40000000 - 0x5fffffff N N  PCI Memory access windows
    0x60000000 - 0x60ffffff N N  PCI IO access window
    0x61000000 - 0x61ffffff N N  PCI config space window
    0x62000000 - 0x6200ffff N N  PCI bridge register window
    0x80000000 - 0x8fffffff N N  SDRAM echo area (used for PCI accesses)

    ARM966E
    -------

    Physical Address Range  C B  Description
    ----------------------- - -  -----------
    0x00000000 - 0x000fffff N N  SSRAM
    0x00100000 - 0x0fffffff N N  SDRAM (depends on part fitted)
    0x10000000 - 0x1fffffff N N  System control and peripheral registers
    0x20000000 - 0x23ffffff N N  Boot ROM (contains boot Monitor)
    0x24000000 - 0x27ffffff N N  FLASH ROM (contains RedBoot)
    0x28000000 - 0x2bffffff N N  SSRAM echo area
    0x40000000 - 0x5fffffff N N  PCI Memory access windows
    0x60000000 - 0x60ffffff N N  PCI IO access window
    0x61000000 - 0x61ffffff N N  PCI config space window
    0x62000000 - 0x6200ffff N N  PCI bridge register window
    0x80000000 - 0x8fffffff N N  SDRAM echo area (used for PCI accesses)

## Rebuilding RedBoot

These shell variables provide the platform-specific information needed for building RedBoot according to the procedure described in Chapter 3:

    export TARGET=integrator
    export ARCH_DIR=arm
    export PLATFORM_DIR=integrator

The names of configuration files are listed above with the description of the associated modes.

Prev | Home | Next
ARM/ARM7 ARM Evaluator7T | Up | ARM/ARM7+ARM9 ARM PID Board and EPI Dev7+Dev9