eCos User Guide
Prev | Appendix A. Target Setup | Next

# Compaq iPAQ PocketPC Hardware Setup

For setting up the iPAQ to run with RedBoot, see the the RedBoot User's Guide. Connections may be made using the Compact Flash Ethernet interface. A serial cable may be connected directly, or via the cradle. Serial communication uses the parameters 38400,8,N,1. The LCD/Touchscreen may also be used as an interface to RedBoot and eCos applications.

Prev | Home | Next
StrongARM EBSA-285 Hardware Setup | Up | SH3/EDK7708 Hardware Setup