eCos User Guide
Prev | Appendix B. Real-time characterization | Next

# Board: NEC VR4373

    Board: NEC VR4373

    CPU  : NEC VR4300 133MHz

    Startup, main stack             : stack used  1304 size  3576
    Startup              :  Interrupt stack used   980 size  4096
    Startup              : Idlethread stack used   494 size  2552

    eCos Kernel Timings
    Notes: all times are in microseconds (.000001) unless otherwise stated

    Reading the hardware clock takes 3 `ticks' overhead
    ... this value will be factored out of all other measurements
    Clock interrupt took    6.49 microseconds (431 raw clock ticks)

    Testing parameters:
       Clock samples:          32
       Threads:                16
       Thread switches:       128
       Mutexes:                32
       Mailboxes:              32
       Semaphores:             32
       Scheduler operations:  128
       Counters:               32
       Alarms:                 32

                                     Confidence
         Ave     Min     Max     Var  Ave  Min  Function
      ======  ======  ======  ====== ========== ========
       17.21   16.18   22.14    0.88   75%  68% Create thread
        0.84    0.78    1.29    0.10   81%  81% Yield thread [all suspended]
        0.90    0.62    3.20    0.35   87%  87% Suspend [suspended] thread
        0.74    0.65    1.16    0.12   81%  68% Resume thread
        1.11    0.90    1.70    0.25   75%  68% Set priority
        0.11    0.05    0.35    0.09   75%  75% Get priority
        2.93    2.24    8.27    0.78   93%  75% Kill [suspended] thread
        0.88    0.78    1.92    0.16   93%  81% Yield [no other] thread
        1.82    1.20    4.71    0.62   87%  62% Resume [suspended low prio] thread
        0.70    0.63    0.86    0.09   68%  68% Resume [runnable low prio] thread
        1.21    1.07    1.61    0.13   81%  68% Suspend [runnable] thread
        0.86    0.78    1.58    0.13   81%  81% Yield [only low prio] thread
        0.69    0.62    0.84    0.09   68%  68% Suspend [runnable->not runnable]
        2.64    2.24    4.35    0.43   81%  62% Kill [runnable] thread
        1.50    1.07    5.82    0.56   93%  87% Destroy [dead] thread
        3.66    2.75    7.74    0.82   50%  56% Destroy [runnable] thread
       13.65    8.33   27.88    3.70   50%  43% Resume [high priority] thread
        2.04    1.89    3.32    0.15   46%  49% Thread switch

        0.19    0.05    0.83    0.13   48%  44% Scheduler lock
        0.50    0.41    1.59    0.13   89%  73% Scheduler unlock [0 threads]
        0.52    0.41    1.29    0.14   89%  64% Scheduler unlock [1 suspended]
        0.56    0.41    1.49    0.15   42%  47% Scheduler unlock [many suspended]
        0.56    0.41    1.41    0.15   43%  47% Scheduler unlock [many low prio]

        0.57    0.20    2.33    0.27   65%  50% Init mutex
        0.89    0.75    3.35    0.20   96%  75% Lock [unlocked] mutex
        0.90    0.74    4.38    0.25   96%  93% Unlock [locked] mutex
        0.77    0.65    2.63    0.17   96%  75% Trylock [unlocked] mutex
        0.66    0.59    1.16    0.10   75%  75% Trylock [locked] mutex
        0.07    0.00    0.45    0.09   75%  75% Destroy mutex
        7.95    7.71    9.49    0.19   50%  46% Unlock/Lock mutex

        1.04    0.81    3.44    0.27   93%  68% Create mbox
        0.10    0.02    0.57    0.11   71%  68% Peek [empty] mbox
        1.15    0.83    4.71    0.31   53%  71% Put [first] mbox
        0.10    0.02    0.57    0.12   68%  68% Peek [1 msg] mbox
        1.01    0.83    3.83    0.22   93%  75% Put [second] mbox
        0.09    0.02    0.57    0.10   71%  71% Peek [2 msgs] mbox
        1.03    0.81    5.02    0.27   96%  87% Get [first] mbox
        0.93    0.81    1.61    0.14   84%  62% Get [second] mbox
        1.07    0.77    4.18    0.23   68%  50% Tryput [first] mbox
        0.89    0.72    3.49    0.21   93%  71% Peek item [non-empty] mbox
        1.04    0.83    4.09    0.26   90%  81% Tryget [non-empty] mbox
        0.79    0.68    1.97    0.15   87%  68% Peek item [empty] mbox
        0.84    0.72    2.36    0.17   93%  68% Tryget [empty] mbox
        0.13    0.02    0.59    0.13   87%  62% Waiting to get mbox
        0.13    0.02    0.90    0.13   90%  62% Waiting to put mbox
        0.93    0.77    3.23    0.21   90%  71% Delete mbox
        4.74    4.51    8.80    0.32   93%  78% Put/Get mbox

        0.50    0.21    1.95    0.29   90%  50% Init semaphore
        0.86    0.57    2.87    0.29   93%  56% Post [0] semaphore
        1.01    0.74    3.62    0.28   93%  56% Wait [1] semaphore
        0.87    0.60    3.17    0.28   90%  59% Trywait [0] semaphore
        0.74    0.62    1.70    0.14   93%  56% Trywait [1] semaphore
        0.36    0.11    1.11    0.26   65%  56% Peek semaphore
        0.25    0.12    1.19    0.14   93%  56% Destroy semaphore
        7.85    7.52    8.93    0.21   62%  43% Post/Wait semaphore

        0.90    0.44    3.08    0.29   65%  28% Create counter
        0.07    0.05    0.89    0.05   96%  96% Get counter value
        0.06    0.05    0.33    0.02   96%  96% Set counter value
        0.88    0.86    1.62    0.05   96%  96% Tick counter
        0.13    0.12    0.41    0.02   96%  96% Delete counter

        1.37    0.81    2.95    0.27   62%  25% Create alarm
        1.35    1.17    6.03    0.31   96%  93% Initialize alarm
        0.11    0.08    0.65    0.05   90%  90% Disable alarm
        1.23    1.14    3.05    0.15   93%  87% Enable alarm
        0.21    0.18    0.47    0.04   90%  90% Delete alarm
        1.03    0.99    2.11    0.07   96%  96% Tick counter [1 alarm]
        4.96    4.96    4.96    0.00  100% 100% Tick counter [many alarms]
        1.70    1.67    2.51    0.05   96%  96% Tick & fire counter [1 alarm]
       26.39   26.38   26.71    0.02   96%  96% Tick & fire counters [>1 together]
        5.65    5.64    5.91    0.02   96%  96% Tick & fire counters [>1 separately]
        2.55    2.38    9.86    0.19   96%  54% Alarm latency [0 threads]
        5.37    3.80    9.73    0.95   50%  34% Alarm latency [2 threads]
        8.79    5.83   16.12    1.29   57%  14% Alarm latency [many threads]

        5.85    2.26   16.24    0.00            Clock/interrupt latency

     1540    1536    1544  (main stack:  1664)  Thread stack used (2552 total)
    All done, main stack            : stack used  1664 size  3576
    All done             :  Interrupt stack used   312 size  4096
    All done             : Idlethread stack used  1440 size  2552

    Timing complete - 23810 ms total

    PASS:<Basic timing OK>
    EXIT:<done>

Prev | Home | Next
Board: Cogent CMA MPC860 (PowerPC) Evaluation | Up | Board: Intel SA1110 (Assabet)