eCos Reference Manual
Prev | Chapter 2. RedBoot Commands and Examples | Next

# Executing Programs from RedBoot

Once an image has been loaded into memory, either via the load command or the fis load command, execution may be transfered to that image.

> NOTE: The image is assumed to be a stand-alone entity, as RedBoot gives the entire platform over to it. Typical examples would be an eCos application or a Linux kernel.

Prev | Home | Next
Persistent State Flash-based Configuration and Control | Up | go