eCos Reference Manual
Prev | Chapter 18. Device Driver Interface to the Kernel | Next

# Device Driver Models

There are several ways in which device drivers may be built. The exact model chosen will depend on the properties of the device and the behavior desired. There are three basic models that may be adopted.

The first model is to do all device processing in the ISR. When it is invoked the ISR programs the device hardware directly and accesses data to be transferred directly in memory. The ISR should also call `cyg_drv_interrupt_acknowledge()`. When it is finished it may optionally request that its DSR be invoked. The DSR does nothing but call `cyg_drv_cond_signal()` to cause a thread to be woken up. Thread level code must call `cyg_drv_isr_lock()`, or `cyg_drv_interrupt_mask()` to prevent ISRs running while it manipulates shared memory.

The second model is to defer device processing to the DSR. The ISR simply prevents further delivery of interrupts by either programming the device, or by calling `cyg_drv_interrupt_mask()`. It must then call `cyg_drv_interrupt_acknowledge()` to allow other interrupts to be delivered and then request that its DSR be called. When the DSR runs it does the majority of the device handling, optionally signals a condition variable to wake a thread, and finishes by calling `cyg_drv_interrupt_unmask()` to re-allow device interrupts. Thread level code uses `cyg_drv_dsr_lock()` to prevent DSRs running while it manipulates shared memory. The eCos serial device drivers use this approach.

The third model is to defer device processing even further to a thread. The ISR behaves exactly as in the previous model and simply blocks and acknowledges the interrupt before request that the DSR run. The DSR itself only calls `cyg_drv_cond_signal()` to wake the thread. When the thread awakens it performs all device processing, and has full access to all kernel facilities while it does so. It should finish by calling `cyg_drv_interrupt_unmask()` to re-allow device interrupts. The eCos ethernet device drivers are written to this model.

The first model is good for devices that need immediate processing and interact infrequently with thread level. The second model trades a little latency in dealing with the device for a less intrusive synchronization mechanism. The last model allows device processing to be scheduled with other threads and permits more complex device handling.

Prev | Home | Next
SMP Support | Up | Synchronization Levels