eCos User Guide
Prev | Chapter 28. Manual Configuration | Next

# Editing the Sources

For many users, controlling the packages and manipulating the available configuration options will be sufficient to create an embedded operating system that meets the application's requirements. However, since eCos is shipped entirely in source form, it is possible to go further when necessary: you can edit the eCos sources themselves. This requires some understanding of the way the eCos build system works.

The most obvious place to edit the source code is directly in the component repository. For example, you could edit the file `kernel/`<version>`/src/sync/mutex.cxx` to change the way kernel mutexes work, or possibly just to add some extra diagnostics or assertions. Once the file has been edited, it is possible to invoke make at the top level of the build tree and the target library will be rebuilt as required. A small optimization is possible: the build tree is largely a mirror of the component repository, so it too will contain a subdirectory `kernel/`<version>``; if make is invoked in this directory then it will only check for changes to the kernel sources, which is a bit more efficient than checking for changes throughout the component repository.

Editing a file in the component repository is fine if this tree is used for only one eCos configuration. If the repository is used for several different configurations, however, and especially if it is shared by multiple users, then making what may be experimental changes to the master sources would be a bad idea. The build system provides an alternative. It is possible to make a copy of the file in the build tree, in other words copy `mutex.cxx` from the `kernel/`<version>`/src/sync` directory in the component repository to `kernel/`<version>`/src/sync` in the build tree, and edit the file in the build tree. When make is invoked it will pick up local copies of any of the sources in preference to the master versions in the component repository. Once you have finished modifying the eCos sources you can install the final version back in the component repository. If the changes were temporary in nature and only served to aid the debugging process, then you can discard the modified version of the sources.

The situation is slightly more complicated for the header files that a package may export, such as the C library’s `stdio.h` header file, which can be found in the directory `language/c/libc/`<version>`/include`. If such a header file is changed, either directly in the component repository or after copying it to the build tree, then make must be invoked at the top level of the build tree. In cases like this it is not safe to rebuild just the C library because other packages may depend on the contents of `stdio.h`.

Prev | Home | Next
Editing an eCos Savefile | Up | Modifying the Memory Layout