eCos User Guide
Prev | Appendix A. Target Setup | Next

# i386 PC Hardware Setup

eCos application on the PC can be run in three ways: via RedBoot, loaded directly from a floppy disk, or loaded by the GRUB bootloader.

## RedBoot Support

For information about setting up the PC to run with RedBoot, consult the RedBoot User"s Guide. If using serial debugging, the serial line runs at 38400 baud 8-N-1 and should be connected to the debug host using a null modem cable. If ethernet debugging is required, an i82559 compatible network interface card, such as an Intel EtherExpress Pro 10/100, should be installed on the target PC and connected to the development PC running GDB. When RedBoot is configured appropriately to have an IP address set, then GDB will be able to debug directly over TCP/IP to the target PC.

## Floppy Disk Support

If an application is built with a startup type of FLOPPY, then it is configured to be a self-booting image that must be written onto a formatted floppy disk. This will erase any existing file system or data that is already on the disk, so proceed with caution.

To write an application to floppy disk, it must first be converted to a pure binary format. This is done with the following command:

    $ i386-elf-objcopy -O binary app.elf app.bin

Here `app.elf` is the final linked application executable, in ELF format (it may not have a `.elf` extension). The file `app.bin` is the resulting pure binary file. This must be written to the floppy disk with the following command:

    $ dd conv=sync if=app.bin of=/dev/fd0

For NT Cygwin users, this can be done by first ensuring that the raw floppy device is mounted as `/dev/fd0`. To check if this is the case, type the command mount at the Cygwin bash prompt. If the floppy drive is already mounted, it will be listed as something similar to the following line:

      \\.\a: /dev/fd0 user binmode

If this line is not listed, then mount the floppy drive using the command:

    $ mount -f -b //./a: /dev/fd0

To actually install the boot image on the floppy, use the command:

    $ dd conv=sync if=app.bin of=/dev/fd0

Insert this floppy in the A: drive of the PC to be used as a target and ensure that the BIOS is configured to boot from A: by default. On reset, the PC will boot from the floppy and the eCos application will load itself and execute immediately.

> NOTE: Unreliable floppy media may cause the write to silently fail. This can be determined if the RedBoot image does not correctly boot. In such cases, the floppy should be (unconditionally) reformatted using the fdformat command on Linux, or format a: /u on DOS/Windows. If this fails, try a different disk.

## GRUB Bootloader Support

If an application is built with the GRUB startup type, it is configured to be loaded by the GRUB bootloader.

GRUB is an open source boot loader that supports many different operating systems. It is available from http://www.gnu.org/software/grub. The latest version of GRUB should be downloaded from there and installed. In Red Hat Linux version 7.2 and later it is the default bootloader for Linux and therefore is already installed.

To install GRUB on a floppy disk from Linux you need to execute the following commands:

    $ mformat a:
    $ mount /mnt/floppy
    $ grub-install --root-directory=/mnt/floppy '(fd0)'
    Probing devices to guess BIOS drives. This may take a long time.
    Installation finished. No error reported.
    This is the contents of the device map /mnt/floppy/boot/grub/device.map.
    Check if this is correct or not. If any of the lines is incorrect,
    fix it and re-run the script `grub-install'.

    (fd0)	/dev/fd0
    $ cp $ECOS_REPOSITORY/packages/hal/i386/pc/current/misc/menu.lst /mnt/floppy/boot/grub
    $ umount /mnt/floppy

The file `menu.lst` is an example GRUB menu configuration file. It contains menu items to load some of the standard eCos tests from floppy or from partition zero of the first hard disk. You should, of course, customize this file to load your own application. Alternatively you can use the command-line interface of GRUB to input commands yourself.

Applications can be installed, or updated simply by copying them to the floppy disk at the location expected by the `menu.lst` file. For booting from floppy disks it is recommended that the executable be stripped of all debug and symbol table information before copying. This reduces the size of the file and can make booting faster.

To install GRUB on a hard disk, refer to the GRUB documentation. Be warned, however, that if you get this wrong it may compromise any existing bootloader that exists on the hard disk and may make any other operating systems unbootable. Practice on floppy disks or sacrificial hard disks first. On machines running Red Hat Linux version 7.2 and later, you can just add your own menu items to the `/boot/grub/menu.lst` file that already exists.

## Debugging FLOPPY and GRUB Applications

When RedBoot loads an application it also provides debugging services in the form of GDB remote protocol stubs. When an application is loaded stand-alone from a floppy disk, or by GRUB, these services are not present. To allow these application to be debugged, it is possible to include GDB stubs into the application.

To do this, set the "Support for GDB stubs" (`CYGDBG_HAL_DEBUG_GDB_INCLUDE_STUBS`) configuration option. Following this any application built will allow GDB to connect to the debug serial port (by default serial device 0, also known as COM1) whenever the application takes an exception, or if a Control-C is typed to the debug port. Ethernet debugging is not supported.

The option "Enable initial breakpoint" (`CYGDBG_HAL_DEBUG_GDB_INITIAL_BREAK`) causes the HAL to take a breakpoint immediately before calling cyg_start(). This gives the developer a chance to set any breakpoints or inspect the system state before it proceeds. The configuration sets this option by default if GDB stubs are included, and this is not a RedBoot build. To make the application execute immediately either disable this option, or disable `CYGDBG_HAL_DEBUG_GDB_INCLUDE_STUBS`.

Prev | Home | Next
NEC CEB-V850/SB1 Hardware Setup | Up | i386/Linux Synthetic Target Setup